|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ABC  Logo 2024.jpg | | | Risk Assessment – Building & Glazing Hazards | | |
| Location: Leys Lane, Attleborough NR17 2HX  Date: December 2024 | | | | | |
| Potential Hazard | Who is at risk? | Existing Control Measure | Risk Rating | Preventative Measures | Responsibilities |
| * Glazed door * Laceration if broken | All Attending the premises including children who could be inclined to run around | All glazed doors which contain specialist safety glass | Low | * Partition glazing contains window glass * All glass panel above waist height | * Deacons * Fabric Officer |
| * Church building and internal premises | All attending premises including older persons with visibility difficulties | Walkways and general access point clear of obstacles  Floor covering in good repair | Med | * Regular inspection of premises 6/12 | * Deacon * Fabric Officer |
| * External premises * gravel access * graveyard and garden | All attending premises  Those who provide maintenance such as grass cutting | Ensure that the property is in good repair  Grave stones are not loose or unstable  Any maintenance equipment is in good state of repair and operator is familiar with use  i.e. grass cutter and garden tools/ladders | Med | * Repair worn or faulty equipment * Provide additional protective clothing i.e. gloves | * Deacons * Fabric Officer |
| * Car parking areas * Collision by moving vehicle | All who visit premises | Identified parking area for people with disability  Surface maintained regularly (re- shingle if required)  Grass area maintained regularly  Movement sensors to lighting in car park area and entrance footpath | Med | * Car Parking area used by authorised persons who attend the building | * Deacons |